# Amiga 4 Joysticks

This adapter will make it possible to connect 2 extra joysticks to the Amiga. This requires that the game is aware of this Multi-Joystick Extender in order to use it. The adapter is connected to the parallelport of the Amiga.

(to the 1st Joystick).
(to the 2nd Joystick).
(to the Computer).

9 PIN D-SUB MALE to the 1st Joystick.
9 PIN D-SUB MALE to the 2nd Joystick.
25 PIN D-SUB MALE to the Parallelcable.

| Parport | Joy 1 | Joy 2
--- | --- | --- | ---
Up 1 | 2 | 1 |
Down 1 | 3 | 2 |
Left 1 | 4 | 3 |
Right 1 | 5 | 4 |
Up 2 | 6 |  | 1
Down 2 | 7 |  | 2
Left 2 | 8 |  | 3
Right 2 | 9 |  | 4
Fire 2 | 11 |  | 6
Fire 1 | 13 | 6 |
Ground 2 | 18 |  | 8
Ground 1 | 19 | 8 |

Contributor: Joakim Ögren, Rob Gill

Source:
Tomi Engdahl's Joystick page

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-07