# Atari Falcon030 DSP Port

26 PIN UNKNOWN 3 ROW FEMALE CONNECTOR on the computer

Pin | Description
--- | ---
1 | General Purpose 0
2 | General Purpose 2
3 | General Purpose 1
4 | SDMA Play Data
5 | SDMA Play Clock
6 | SDMA Play Sync
7 | Not Connect
8 | Ground
9 | +12V
10 | Ground
11 | Sync Serial I/F Ctrl 0
12 | Sync Serial I/F Ctrl 1
13 | Sync Serial I/F Ctrl 2
14 | Ground
15 | Sync Serial Data In
16 | Ground
17 | +12V
18 | Ground
19 | SDMA Record Data
20 | SDMA Record Clock
21 | SDMA Record Sync
22 | DSP Interrupt
23 | Sync Serial I/F Data Out
24 | Sync Serial I/F Clock
25 | Ground
26 | External Clock Input

Contributor: Joakim Ögren, Jan Krupka

Source:
Atari Falcon030 DSP pinout at Technick.net

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-08