# PGA

Videotype: Analogue.

(at the videocard)
(at the monitor cable)

9 PIN D-SUB FEMALE at the videocard.
9 PIN D-SUB MALE at the monitor cable.

Pin | Name | Description
--- | --- | ---
1 | R | Red
2 | G | Green
3 | B | Blue
4 | CSYNC | Composite Sync
5 | MODE | Mode Control
6 | RGND | Red Ground
7 | GGND | Green Ground
8 | BGND | Blue Ground
9 | GND | Ground

Contributor: Joakim Ögren

Source:
?

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-07