# DEC Printer

(at ???)
(at ???)

37 PIN D-SUB FEMALE at ???.
37 PIN D-SUB MALE at ???.

Pin | Name | Dir | Description
--- | --- | --- | ---
1 | DAT<3> |  | Data Bit 3
2 |  |  | Not available
3 |  |  | Not available
4 |  |  | Not available
5 | DAT<6> |  | Data Bit 6
6 | DAT<7> |  | Data Bit 7
7 |  |  | Not available
8 | Strobe |  | Data Bit 1
9 |  |  | Not available
10 |  |  | Not available
11 |  |  | Not available
12 | On Line |  | Strobe
13 |  |  | Not available
14 | Connection |  | Connection
15 |  |  | Not available
16 |  |  | Not available
17 | DAVFU |  | DAVFU
18 | Demand |  | Data Bit 0
19 |  |  | Not available
20 | DAT<1> |  | Data Bit 2
21 |  |  | Not available
22 | DAT<2> |  | Data Bit 2
23 | DAT<4> |  | Data Bit 4
24 | DAT<5> |  | Data Bit 5
25 |  |  | Not available
26 | DAT<0> |  | Data Bit 2
27 | Ground |  | Ground
28 | Ground DAT<0> |  | Ground Data Bit 0
29 | Ground DAT<1> |  | Ground Data Bit 1
30 | Ground DAT<2> |  | Ground Data Bit 2
31 | Ground DAT<3> |  | Ground Data Bit 3
32 | Ground DAT<4> |  | Ground Data Bit 4
33 | Ground DAT<5> |  | Ground Data Bit 5
34 | Ground DAT<6> |  | Ground Data Bit 6
35 | Ground DAT<7> |  | Ground Data Bit 7
36 |  |  | Not available
37 |  |  | Not available

Note: Direction is Host (Computer) relative Peripheral (Printer).

Contributor: Joakim Ögren

Source:
?

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-07