# SUN Power

18 PIN MOLEX 39-29-9182 CONNECTOR at the motherboard

Available on the SUN SPARCengine 5 motherboard

Pin | Description
--- | ---
1 | +12
2 | -12
3 | +5
4 | +5
5 | +5
6 | +5
7 | +5
8 | +5
9 | Power off
10 | Ground
11 | Ground
12 | Ground
13 | Ground
14 | Ground
15 | Ground
16 | AC Outlet
17 | Fan
18 | Power on

Contributor: Joakim Ögren

Source:
SUN SPARCengine 5 manual at SUN manuals site

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-07