# C128 RGBI

(at the Computer)

9 PIN D-SUB FEMALE at the Computer.

Pin | Name | Dir | Description
--- | --- | --- | ---
1 | GND |  | Ground
2 | GND |  | Ground
3 | R |  | Red
4 | G |  | Green
5 | B |  | Blue
6 | I |  | Intensity
7 | VIDEO |  | Composite Video
8 | HSYNC |  | Horizontal Sync
9 | VSYNC |  | Vertical Sync

Note: Direction is Computer relative Monitor.

Contributor: Joakim Ögren

Source:
Usenet posting in comp.sys.cbm, C128 screen cables by Marko Makela

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-08