# SUN SROMBO

Available on SUN SPARCengine motherboards
Seems to be for SUN internal factory tests/programming

(at the motherboard)

34 PIN IDC MALE at the motherboard

Pin | Name
--- | ---
1 | ADR19
2 | VCC
3 | ADR16
4 | ADR18
5 | ADR15
6 | ADR17
7 | ADR12
8 | ADR14
9 | ADR7
10 | ADR13
11 | ADR6
12 | ADR8
13 | ADR5
14 | ADR9
15 | ADR4
16 | ADR11
17 | ADR3
18 | RD_L
19 | ADR2
20 | ADR10
21 | ADR1
22 | ROMBO_CS_L
23 | ADR0
24 | DAT7
25 | DAT0
26 | DAT6
27 | DAT1
28 | DAT5
29 | DAT2
30 | DAT4
31 | GND
32 | DAT3
33 | NC
34 | WR_L

Contributor: Joakim Ögren

Source:
SUN SPARCengine Ultra AXmp Manual

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-07