# Sun Aux Power

Available on SUN SPARCengine motherboards

(at the motherboard)

24 PIN MOLEX 39-29-9242 at the Motherboard

Pin | Name
--- | ---
1 | +3.3V
2 | GND
3 | +3.3V
4 | GND
5 | +3.3V
6 | GND
7 | +3.3V
8 | GND
9 | PWR_SENSE_3.3V
10 | GND
11 | PWR_SENSE_GND
12 | +12V
13 | +5V
14 | GND
15 | +5V
16 | GND
17 | +5V
18 | GND
19 | +5V
20 | GND
21 | PWR_SENSE_5V
22 | GND
23 | PWR_SENSE_GND
24 | -12V

Contributor: Joakim Ögren

Source:
SUN SPARCengine Ultra AXmp Manual

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-08