# Psion Organiser II Connector Top Slot (D)

16 PIN UNKNOWN CONNECTOR on the PDA

Pin | Name | Description
--- | --- | ---
1 | SD7 | Data Bit 7
2 | SD0 | Data Bit 0
3 | SD6 | Data Bit 6
4 | SD1 | Data Bit 1
5 | SD5 | Data Bit 5
6 | SD2 | Data Bit 2
7 | SD4 | Data Bit 4
8 | SD3 | Data Bit 3
9 | GND | 0 Volts
10 | SCK | Undefined Control Line
11 | SVB | External Power Input / Battery Output Voltage - 0.6 Volt
12 | SS3 | Slot Select 3
13 | SCVV | +5 Volts
14 | AC | External On/Clear
15 | SOME | Undefined Control Line
16 | SMR | Undefined Control Line

Contributor: Joakim Ögren

Source:
Atari Falcon030 DSP pinout at Technick.net

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-08