# C16/C116/+4 Cassette

Available on the Commodore C16, C116 and +4 computers.

(at the computer)

7 PIN MINI-DIN FEMALE at the computer.

Pin | Name | Dir | Description
--- | --- | --- | ---
1 | GND |  | Ground
2 | +5V |  | +5 Volts DC
3 | MOTOR |  | Cassette Motor
4 | READ |  | Cassette Read
5 | WRITE |  | Cassette Write
6 | SENSE |  | Cassette Sense
7 | GND |  | Ground

Note: Direction is Computer relative Cassette.

Contributor: Joakim Ögren, Arwin Vosselman

Source:
SAMS Computerfacts CC8 Commodore 16

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-07