# Apple Digital Audio/Video (DAV)

60 PIN UNKNOWN CONNECTOR

The Audio/Video Input/Output Card has a separate connector called the DAV (digital audio video) connector. The DAV connector provides access to the Audio/Video card's 4:2:2 unscaled YUV video input data bus and associated control signals. By means of a 60-pin cable to the DAV connector, a PCI expansion card can gain access to the digital video bus on the Audio/Video Input/Output Card and use it to transfer real-time video data to the computer. Such a PCI expansion card can contain a hardware video compressor or other video processor.

The DAV connector accepts YUV video and analog sound from the PCI expansion card.

The 60-pin DAV connector is located at the top edge of the Audio/Video Input/Output Card. A PCI expansion card that uses the DAV interface can be connected to the Audio/Video Input/Output Card with a 7-inch 60-conductor flat-ribbon cable.

Pin | Description
--- | ---
1 | Ground
2 | Reserved (or GeoPort Clock)
3 | Ground
4 | Reserved (or LLC_OUT)
5 | Ground
6 | Reserved (or PXQ_OUT)
7 | Ground
8 | Reserved (or VS_OUT)
9 | Ground
10 | Reserved (or HS_OUT)
11 | UV bit 7
12 | UV bit 6
13 | UV bit 5
14 | UV bit 4
15 | UV bit 3
16 | UV bit 2
17 | UV bit 1
18 | UV bit 0
19 | Y bit 7
20 | Y bit 6
21 | Y bit 5
22 | Y bit 4
23 | Y bit 3
24 | Y bit 2
25 | Y bit 1
26 | Y bit 0
27 | Ground
28 | Line-locked clock (LLC) in
29 | Ground
30 | Clock reference qualifier (PXQ) In
31 | Ground
32 | Vertical sync (VS) In
33 | Ground
34 | Reserved (or Horizontal Sync (HS) In)
35 | Ground
36 | HRef In
37 | Ground
38 | DIR * (or FLD)
39 | IIC Data *
40 | IIC Clock
41 | Ground
42 | Analog audio input left
43 | Analog audio input common
44 | Analog audio input right
45 | Ground
46 | Digital audio input
47 | Ground
48 | Digital audio output
49 | Ground
50 | Digital audio clock
51 | Ground
52 | Digital audio sync
53 | Ground
54 | S video input C component
55 | Video input ground
56 | S video input Y component
57 | Video input ground
58 | Reserved
59 | Reserved
60 | Reserved

Contributor: Joakim Ögren

Source:
Apple Tech Info Library 18547: Power Macintosh 7200, 7500, 8500, 9500 Pinouts at Apple TIL homepage

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2000-07-09