# Amstrad CPC6128 Diskdrive 2

(at the computer)

34 PIN MALE EDGE at the computer.

Pin | Name
--- | ---
1 | READY
2 | GND
3 | SIDE 1 SELECT
4 | GND
5 | READ DATA
6 | GND
7 | WRITE PROTECT
8 | GND
9 | TRACK 0
10 | GND
11 | WRITE GATE
12 | GND
13 | WRITE DATA
14 | GND
15 | STEP
16 | GND
17 | DIRECTION SELECT
18 | GND
19 | MOTOR ON
20 | GND
21 | n/c
22 | GND
23 | DRIVE SELECT 1
24 | GND
25 | n/c
26 | GND
27 | INDEX
28 | GND
29 | n/c
30 | GND
31 | n/c
32 | GND
33 | n/c
34 | GND

Contributor: Joakim Ögren, Agnello Guarracino

Source:
Amstrad CPC6128 User Instructions Manual

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-07