# Commodore 1084d & 1084dS

(at the Monitor)

9 PIN D-SUB FEMALE at the Monitor.

Pin | Name | Analog Mode | Digital Mode
--- | --- | --- | ---
1 | GND | Ground | Ground
2 | GND | Ground | Ground
3 | R | Red | Red
4 | G | Green | Green
5 | B | Blue | Blue
6 | I | n/c | Intensity
7 | CSYNC | Composite Sync | n/c
8 | HSYNC | n/c | Horizontal Sync
9 | VSYNC | n/c | Vertical Sync

Contributor: Joakim Ögren

Source:
National Amiga's C1084d page

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-07