# Atari 5200 Joystick

(at the Atari)

UNKNOWN CONNECTOR at the Atari.

Pin | Description
--- | ---
1 | Keypad -- right column
2 | Keypad -- middle column
3 | Keypad -- left column
4 | Start, Pause, and Reset common
5 | Keypad -- third row and Reset
6 | Keypad -- second row and Pause
7 | Keypad -- top row and Start
8 | Keypad -- bottom row
9 | Pot common
10 | Horizontal pot (POT0, 2, 4, 6)
11 | Vertical pot (POT1, 3, 5, 7)
12 | 5 volts DC
13 | Bottom side buttons (TRIG0, 1, 2, 3)
14 | Top side buttons
15 | 0 volts -- ground

Contributor: Joakim Ögren, Eric Parent

Source:
Classic Atari 2600/5200/7800 Game Systems FAQ

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-08