# IEEE1284-C

36 PIN HI-DENSITY CENTRONICS???

Pin | Name | Dir | Description
--- | --- | --- | ---
1 | Busy |  | Busy
2 | Select |  | Select
3 | /nAck |  | Acknowledge
4 | /nFault |  | Error
5 | PError |  | Paper End
6 | data0 |  | Address, Data or RLE Data Bit 0
7 | data1 |  | Address, Data or RLE Data Bit 1
8 | data2 |  | Address, Data or RLE Data Bit 2
9 | data3 |  | Address, Data or RLE Data Bit 3
10 | data4 |  | Address, Data or RLE Data Bit 4
11 | data5 |  | Address, Data or RLE Data Bit 5
12 | data6 |  | Address, Data or RLE Data Bit 6
13 | data7 |  | Address, Data or RLE Data Bit 7
14 | /nInit |  | Initialize
15 | nStrobe |  | Strobe
16 | /nSelectIn |  | Select In
17 | /nAutoFd |  | Autofeed
18 | GND |  | Signal Ground
19 | GND |  | Signal Ground
20 | GND |  | Signal Ground
21 | GND |  | Signal Ground
22 | GND |  | Signal Ground
23 | GND |  | Signal Ground
24 | GND |  | Signal Ground
25 | GND |  | Signal Ground
26 | GND |  | Signal Ground
27 | GND |  | Signal Ground
28 | GND |  | Signal Ground
29 | GND |  | Signal Ground
30 | GND |  | Signal Ground
31 | GND |  | Signal Ground
32 | GND |  | Signal Ground
33 | GND |  | Signal Ground
34 | GND |  | Signal Ground
35 | GND |  | Signal Ground
36 | GND |  | Signal Ground

Note: Direction is Computer relative Device.

Contributor: Joakim Ögren, Marco Furter

Source:
Microsoft MSDN Library: Extended Capabilities Port Specs

Info: Microsoft MSDN Library

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2000-07-16