# NeoGeo to SCART

(To the Computer)
(to the TV)

8 PIN DIN (DIN45326) MALE to the Computer.
21 PIN SCART MALE to the TV

| NeoGeo | TV |
--- | --- | --- | ---
Audio Out | 1 | 6+2 | Audio In Left+Right
Ground | 2 | 18 | Blanking Signal Ground
Composite Video Out | 3 | 20 | Composite Video In
? | 4 | 16 | Blanking Signal
Green | 5 | 11 | RGB Green In
Red | 6 | 15 | RGB Red In
Blue | 8 | 7 | RGB Blue In

Contributor: Joakim Ögren, Enzo, Steffen Kupfer

Source:
?

Copyright © The Hardware Book Team 1996-2001.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2001-06-07